127(7KLVLVDJHQHULFPDQXDO,WHPVVKRZQPD\QRWDSSO\WR\RXUYDFXXP 3OHDVHFRQWDFWFXVWRPHUVHUYLFHZLWKTXHVWLRQV

**ATTENTION!**

**Read** **all** **safety** **rules** **careful-ly** **before** **attempting** **to** **oper-ate.** **Retain** **for** **future** **reference.**

**DANGER!**

**Never** **operate** **this** **unit** **when** **flammable** **materials** **or** **vapors** **are** **present** **because** **electrical** **devices** **produce** **arcs** **or** **sparks** **that** **can** **cause** **a** **fire** **or** **explo-sion.**

**NEVER** **OPERATE** **UNATTENDED!**

**WARNING!**

**Do** **NOT** **use** **this** **vacuum** **cleaner** **to** **vacuum** **lead** **paint** **debris** **because** **this** **may** **disperse** **fine** **lead** **particles** **into** **the** **air.** **This** **vacuum** **cleaner** **is** **not** **intended** **for** **use** **under** **EPA** **Regulation**

**40** **CFR** **Part** **745** **for** **lead** **paint** **material** **cleanup.**

**SHOP-VAC** **CORPORATION** 2323 Reach Road, P.O. Box 3307 Williamsport, PA 17701-0307 (570) 326-3557

Web site: www.shopvac.com

**SHOP-VAC** **CANADA** 1770 Appleby Line Burlington, Ontario L7L 5P8 (905) 335-9730

Web site: www.shopvac.ca

**Shop** **Vac-México,** **S.A.** **de** **C.V.** Calle Niños Héros #1553 Colonia Agua Blanca

45235 - Zapopan, Jalisco 52 (33) 3188 6388

**Patents** **Issued** **and** **Pending.Printed** **in** **U.S.A.**

**©** **2010** **Shop-Vac** **Corporation.** **All** **rights** **reserved.**

MSC1896

**IMPORTANT** **SAFETY** **INSTRUCTIONS**

When using an electrical appliance, basic precautions should always be followed, including the following:**READ** **ALL** **INSTRUCTIONS** **BEFORE** **USING** **THIS** **APPLIANCE.**

13. Turn off all controls before unplugging.

14. Use extra care when cleaning on stairs.

**WARNING–** **TO** **REDUCE** **THE** **RISK** **OF** **FIRE,** **ELECTRIC** **SHOCK** **OR** **INJURY:**

1. Do not leave appliance when plugged in. Unplug from outlet when not in use and before servicing. Connect to a properly grounded outlet only. See Grounding Instructions.

2. Do not expose to rain – store indoors.

3. Do not allow to be used as a toy. Close attention is necessary when used by or near children. 4. Use only as described in this manual. Use only Manufacturer’s recommended attachments.

5. Do not use with damaged cord or plug. If appliance is not working as it should, has been dropped, damaged, left outdoors or dropped into water, contact Shop-Vac Corporation for assistance.

6. Do Not: pull or carry by cord, use cord as a handle, close a door on cord or pull cord around sharp edges or corners. Do not run appliance over cord. Keep cord away from heated sur-faces.

7. Do not unplug by pulling on cord.To unplug, grasp the plug; not the cord.

8. Do not handle plug or appliance with wet hands.

15. Do not use to pick up flammable or combustible liquids such as gasoline or use in areas where they may be present.

16. Do not use your cleaner as a sprayer of flammable liquids such as oil base paints, lacquers, household cleaners, etc.

17. Do not vacuum toxic, carcinogenic, combustible or other hazardous materials such as asbestos, arsenic, barium, beryllium, lead, pesticides or other health endangering materials. Specially designed units are available for these purposes.

18. Do not pick up soot, cement, plaster or drywall dust without cartridge filter and collection filter bag in place.These are very fine particles that may pass through the foam and affect the performance of the motor or be exhausted back into the air. Additional collection filter bags are available.

19. Do not leave the cord lying on the floor once you have finished the cleaning job. It can become a tripping hazard.

20. Use special care when emptying heavily loaded tanks.

21. To avoid spontaneous combustion, empty tank after each use.

22. The operation of a utility vac can result in foreign objects being blown into eyes, which can result in eye damage. Always wear safety goggles when operating vacuum.

9. Do not put any object into openings. Do not use with any openings blocked; keep free of dust, lint, hair and anything that may reduce air flow.

10. Keep hair, loose clothing, fingers and all parts of body away from openings and moving parts. 11. Do not pick up anything that is burning or smoking, such as cigarettes, matches or hot ashes.

12. Do not use without dust bag and/or filters in place.

23. STAYALERT. Watch what you are doing and use common sense. Do not use vacuum cleaner when you are tired, distracted or under the influence of drugs, alcohol or medication causing diminished control.

24. **WARNING!** Do **NOT** use this vacuum cleaner to vacuum lead paint debris because this may disperse fine lead particles into the air. This vacuum cleaner is not intended for use under EPA Regulation 40 CFR Part 745 for lead paint material cleanup.

**SAVE** **THESE** **INSTRUCTIONS**

**WARNING–** **DO** **NOT** **LEAVE** **VACUUM** **UNATTENDED** **WHEN** **IT** **IS** **PLUGGED** **IN** **AND/OR** **OPERATING.** **UNPLUG** **UNIT** **WHEN** **NOT** **IN** **USE.**

**GROUNDING** **INSTRUCTIONS**

This appliance must be grounded. If it should malfunction or breakdown, grounding provides a path of least resistance for electric current to reduce the risk of electric shock.This appliance is equipped with a cord having an equipment-grounding conductor and grounding plug.The plug must be inserted into an appropriate outlet that is properly installed and grounded in accordance with all local codes and ordinances.

**WARNING–** **IMPROPER** **CONNECTION** **OF** **THE** **EQUIPMENT-GROUNDING** **CONDUCTOR** **CAN** **RESULT** **IN** **A** **RISK** **OF** **ELECTRIC**

**SHOCK.** **CHECK** **WITH** **A** **QUALIFIED** **ELECTRICIAN** **OR** **SERVICE** **PERSON** **IF** **YOU** **ARE** **IN** **DOUBT** **AS** **TO** **WHETHER** **THE** **OUTLET** **IS** **PROPERLY** **GROUNDED.** **DO** **NOT** **MODIFY** **THE** **PLUG** **PROVIDED** **WITH** **THE** **APPLIANCE** **–** **IF** **IT** **WILL** **NOT** **FIT** **THE** **OUTLET,** **HAVE** **A** **PROPER** **OUTLET** **INSTALLED** **BY** **A** **QUALIFIED** **ELECTRICIAN.**

This appliance is for use on a nominal 120-volt circuit, and has a grounded plug that looks like

the plug illustrated in sketch A. A temporary adapter that looks like the adapter illustrated in sketches B and C may be used to connect this plug to a 2-pole receptacle as shown in sketch B if a properly grounded outlet is not available. The temporary adapter should be used only until a properly grounded outlet (sketch A) can be installed by a qualified electrician. The green colored rigid ear, lug or the

like extending from the adapter must be connected to a permanent ground such as a properly grounded outlet box cover.Whenever the adapter is used, it must be held in place by a metal screw.

IN CANADA, THE USE OF A TEMPORARY ADAPTER IS NOT PERMITTED BY THE CANADIAN ELECTRICAL CODE. Make sure that the appliance is connected to an outlet having the same configuration as the plug. No adapter should be used with this appliance.

**EXTENSION** **CORDS**

When using the appliance at a distance where an extension cord becomes necessary, a 3-con-ductor grounding cord of adequate size must be used for safety, and to prevent loss of power and overheating. Use the table below to determine A.W.G. wire size required.To determine ampere rating of your vacuum, refer to nameplate located on rear of motor cover.

Before using appliance, inspect power cord for loose or exposed wires and damaged insulation. Make any needed repairs or replacements before using your appliance. Use only three-wire out-door extension cords which have three-prong grounding-type plugs and three-pole receptacles which accept the extension cord’s plug. When vacuuming liquids, be sure the extension cord connection does not come in contact with the liquid.

**NOTE:** STATIC SHOCKS ARE COMMON IN DRY AREAS OR WHEN THE RELATIVE HUMID-ITY OF THE AIR IS LOW. THIS IS ONLY TEMPORARY AND DOES NOT AFFECT THE USE OF THE APPLIANCE.TO REDUCE THE FREQUENCY OF STATIC SHOCKS IN YOUR HOME, THE BEST REMEDY IS TO ADD MOISTURE TOTHE AIR WITH A CONSOLE OR INSTALLED HUMIDIFIER.

**UNPACKING**

1. Remove vacuum cleaner and all accessories from the carton.

2. Important: Open tank cover by pushing latches or clamps outward with thumbs and remove any accessories that may have been shipped in the tank.

3. Assemble dolly or caster system following instructions.

4. Before replacing cover, please refer to Dry Pick up or Wet Pick up operation to ensure proper filter installation.

5. Replace cover and make sure latches or clamps are secured over raised area of tank cover.

**I=ON,** **O=OFF**

**TOP** **HANDLE** **ASSEMBLY** **(Not** **standard** **with** **all** **models)**

To attach top handle, align holes in handle and holes in tank cover and secure with screws provided **(Figure** **1).**

**ASSEMBLY**

5. Insert casters into feet by placing stem of caster into holes provided. Apply pressure and twisting motion until casters snap into place **(Figure** **23)**. Return tank to upright position.

**1** **19**

**B**

**TOOL** **HOLDER** **ASSEMBLY** **(Not** **standard** **with** **all** **models)**

1. With rear of unit facing you, take tool holder and position it with tabs facing rear of unit **(Figure** **2).**

2. Place “J” shaped tabs into the slots on cord wraps **(Figure3).** 3. Press down until tabs snap into place.

4. Press down on center of tool holder until tab latches on bottom of lid **(Figure** **4).**

**23**

**With** **Rear** **Caster** **Dolly/Tool** **Holder**

You will find four casters **(Figure** **24)**, two caster feet **(Figure** **25)**, rear caster dolly/tool holder **(Figure** **26)**, and four screws with your wet/dry vacuum. Assemble as follows:

**24** **25** **26**

**2** **3** **4**

**CASTER** **SYSTEM** **ASSEMBLY**

***1RW*** ***DOO*** ***XQLWV*** ***DUH*** ***HTXLSSHG*** ***ZLWK*** ***WKH*** ***VDPH*** ***FDVWHU*** ***V\VWHP*** ***)ROORZ*** ***WKH*** ***LQVWUXFWLRQVZKLFKDSSO\WR\RXUVSHFLILFXQLW***

**Without** **Caster** **Feet**

You will find four casters **(Figure** **5)** with your wet/dry vacuum. Assemble as follows:

1. With cord disconnected from receptacle and tank cover removed, turn tank upside down so that bottom is facing up. **5** **6**

2. Insert casters into bottom of tank by placing stem of caster into holes provided. Apply pressure and twisting motion until casters snap into place **(Figure** **6)**.

3. Return tank to upright position.

**5-8** **U.S.** **Gallons** **(18.9** **-** **30.2L)** **With** **Caster** **Feet**

You will find four caster feet **(Figure** **7)**, four casters **(Figure** **8)**, and four screws with your wet/ dry vacuum. Assemble as follows:

1. With cord disconnected from receptacle and tank cover removed, turn tank **7** upside down so that bottom is facing up.

2. Remove any webbing that attaches the caster feet to each other.

3. With front of tank inlet facing you, take caster feet marked with the letter A **(Figure** **9)** and insert stem of caster foot into holes on left front and right rear of tank also marked with letter A **(Figure** **10).**Make sure caster feet are fully inserted into tank bottom and secure with screws provided **(Figure** **11).**

4. Take caster feet marked with the letter B **(Figure** **12)** and insert stem of caster foot into holes on right front and left rear of tank also marked with the letter B **(Figure** **13).** Make sure caster feet are fully inserted into tank bottom and secure with screws provided **(Figure** **14).**

5. Insert casters into feet by placing stem of caster into holes provided. Apply pressure and twisting motion until casters snap into place **(Figure** **15)**.

6. Return tank to upright position.

**11**

1. With cord disconnected from receptacle and tank cover removed, turn tank upside down so that the bottom is facing up.

2. Take rear caster dolly and place into slots (on rear of tank, opposite of drain) and secure with screws provided **(Figure** **27)**.

3. If flat washers are included in hardware package place flat washer over stem of caster before installing casters into feet.**NOTE** **:** Flat washers are not required with all units.

4. Insert casters into bottom of rear caster dolly by placing stem of caster into holes provided. Apply pressure and twisting motion until casters snap into place **(Figure** **28)**.

5. With tank drain facing you, take caster foot marked with the letter A **(Figure** **29)** and place in slot on left side of tank also marked with the letter A. Secure with screw provided **(Figure** **30)**.

6. Take caster foot marked with the letter B **(Figure** **31)** and place in slot on right side of tank also marked with the letter B. Secure with screw provided **(Figure** **32)**.

7. Insert casters into feet by placing stem of casters into holes provided. Apply pressure and twisting motion until casters snap into place **(Figure** **33)**.

8. Return tank to upright position.

9. Place tool basket **(not** **standard** **with** **all** **models)** with curved surface against tank on rear caster dolly assembly **(Figure** **34)**.

**(Not** **standard** **with** **all** **models)** **35** You will find four casters, two caster feet, an accessory caddy and four screws

with your wet/dry vacuum.

**15**

**10** **U.S.** **Gallons** **(37.8L)** **and** **Up** **With** **Caster** **Feet**

You will find four caster feet, four casters and four screws **(Figure** **16)** with your wet/dry vacuum. Assemble as follows:

1. With cord disconnected from receptacle and tank cover removed, turn tank upside down so that bottom is facing up.

2. With front of tank facing you, take caster feet marked with the letter A **(Figure** **17)** and place in slots on left front and right rear of tank also marked with the letter A **(Figure** **18)**. Secure with screws provided **(Figure** **19)**.

3. Take caster feet marked with the letter B **(Figure** **20)** and place in slots on right front and left rear of tank also marked with the letter B **(Figure** **21)**. Secure with screws provided **(Figure** **22)**.

4. If flat washers are included in hardware package place flat washer over stem of caster before installing casters into feet.**NOTE:** Flat washers are not required with all units.

If your accessory caddy looks like the one pictured in **(Figure** **35)** assemble as follows.

1. With cord disconnected from receptacle and tank cover removed, turn tank upside down so that the bottom is facing up.

2. Insert two caster feet into adjacent slots at front of tank. Secure with screws provided.

3. Take accessory caddy and place into remaining slots at back of tank. Secure with screws provided **(Figure** **36)**.

4. Install casters into caddy and feet by inserting the caster stems into the holes provided. Apply pressure and twisting motion until casters snap into place.

If your accessory caddy looks like the one pictured in **(Figure** **37)** assembly as follows.

1. With cord disconnected from receptacle and tank cover removed, turn tank upside down so that the bottom is facing up.

2. Take accessory caddy and place into slots (on rear of tank opposite of drain). Secure with screws provided **(Figure** **38)**.

3. With tank drain facing you, take caster foot marked with the letter A **(Figure** **39)** and place in slot on left side of tank also marked with the letter A. Secure with screw provided **(Figure** **40)**.

4. Take caster foot marked with the letter B **(Figure** **41)** and place in slot on right side of tank also marked with the letter B. Secure with screw provided **(Figure** **42)**.

5. If flatwashers are included in hardware package place flatwasher over stem of caster before installing casters into feet or accessory caddy. **NOTE:** Flatwashers are not required with all units.

6. Install casters into caster feet and accessory caddy by inserting the caster stems into the holes provided. Apply pressure and twisting motion until caster snap into place **(Figure** **43** **&** **44)**. **37** **38** **39** **40**

**59** **60** **61**

**62** **63** **64**

**A**

**A**

**41** **42** **43** **44** **TOOL** **HOLDER** **ASSEMBLY**

**A**

**B**

**A** **B**

**REAR** **WHEEL** **DOLLY/TOOL** **HOLDER** **AND** **FRONT** **CASTER** **FEET** **ASSEMBLY**

**(Not** **standard** **with** **all** **models)**

1. Replace tank cover and apply pressure with thumbs to each latch until it snaps tightly in place. Make sure both lid latches are clamped securely.

2. With rear of unit facing you, take tool holder and position it with the tabs facing rear tank cover **(Figure** **65).**

3. Press tabs of tool holder into the slots on mounting lugs on rear of tank cover **(Figure** **66).**

4. Press down until tabs snap into place.

**66**

You will find two casters **(45)**, two large rear wheels **(46)**, one axle **(47)**, rear dolly/ basket **(48)**, two caster feet **(49)** and four screws with your wet/dry vacuum. Assemble as follows:

**45** **46** **47** **48** **49**

1. With cord disconnected from receptacle and tank cover removed, turn tank upside down so that the bottom is facing up.

2. Place axle upright on a hard surface and hammer on (1) cap nut. Place (1) wheel on axle and slide down to cap nut **(Figure** **50).** Be sure flat side of wheel hub is facing outward.

3. Slide axle through holes provided in dolly/basket **(Figure** **51).**

4. Slide remaining wheel onto axle and hammer on second cap nut **(Figure** **52).**

5. Take rear dolly assembly and place into slots (on rear of tank opposite drain) and secure with screws provided **(Figure** **53).**

6. With tank drain facing you, take caster foot marked with the letter A **(Figure** **54)** and place in slot on left side of tank also marked with the letter A and secure with screw provided **(Figure** **55)**.

7. Take caster foot marked with the letter B **(Figure** **56)** and place in slot on right side of tank also marked with the leter B and secure with screw provided **(Figure** **57)**.

8. Insert casters into feet by placing stem of caster into holes provided. Apply **50** pressure and twisting motion until casters snap into place **(Figure** **58).**

9. Return tank to upright position.

**51** **52** **53** **54**

**NOTE:** **TOOL** **HOLDER** **NOT** **COMPATIBLE** **WITH** **ACCESSORY** **BASKET.**

**ACCESSORY** **BASKET** **ASSEMBLY** **(Not** **standard** **with** **all** **models)**

1. With rear of tank facing you, take accessory basket and position with tabs facing rear of tank **(Figure** **67).**

2. Insert tabs of accessory basket into slots on rear of tank **(Figure** **68).**

3. Press down until basket is secured into place.

**DOLLY** **AND** **CASTER** **ASSEMBLY** **FOR** **All** **AROUND** **PLUS®** **SERIES**

You will ﬁnd four casters **(Figure** **69)** and one dolly **(Figure** **70)** with your wet/dry vacuum. Assemble as follows:

**69** **70**

1. With cord disconnected from receptacle and tank cover removed, turn tank upside down so that bottom is facing up.

2. Take dolly and slide onto bottom of tank making sure to line up screw holes on dolly with screw holes on tank. Secure with screws provided **(Figure** **71).**

3. Install casters into dolly by inserting the caster stems into the holes provided. Apply pres-sure and twisting motion until the casters snap into place **(Figure** **72).**

4. Return tank to upright position.

**71** **72**

**55** **56** **57** **58**

**ASSEMBLY** **FOR**

**All** **AROUND** **PLUS®** **SERIES**

You will find two casters **(a),** two axle housings **(b),** two wheel plugs **(c),** two wheels **(d)**, and two screws with your wet/dry vacuum. Assemble as follows:

**a** **b** **c** **d**

1. With cord disconnected from receptacle and tank cover removed, turn tank upside down so that the bottom is facing up with the inlet towards you **(Figure** **59).**

2. Insert casters into bottom of tank by placing stem of caster into holes provided. Apply pres-sure and twisting motion until casters snap into place **(Figure** **60).**

3. Mount wheel onto axle with smooth face of wheel outward **(Figure** **61).**

4. Insert wheel plug through wheel and axle housing turning wheel plug until it seats flush with outside of wheel **(Figure** **62).**

5. Insert screw provided through back of axle housing **(Figure** **63).**

6. Slide axle housing into dovetail slot at rear of tank: axle housing is tapered and should slide into dovetail slot without excessive force **(Figure** **64).**Tighten screw.

7. Repeat steps 3 through 6 for other wheel assembly. 8. Return tank to upright position.

**CASTER** **FEET** **AND** **CASTER** **ASSEMBLY** **FOR** **METAL** **TANKS**

**(Not** **standard** **with** **all** **models)**

1. With cord disconnected from receptacle and tank cover removed, turn tank upside down so that the bottom is facing up.

2. With a pair of scissors, trim the enclosed template to ﬁt your size tank. Sizes will be 11”, 14” or 16” diameters.

3. Once template is cut out, place on bottom of tank. Align inlet arrow on template with center of inlet on tank **(Figure** **73)**.

4. If caster feet are attached together, separate by remov-ing webbing.

5. Take caster foot marked with the letter A and align arrow on foot **(Figure** **74)** with arrow on template also marked with the letter A **(Figure** **75)**.

6. Place groove of foot over rim of tank and push until the caster foot is tight against bottom of tank **(Figure** **76)**.

7. Secure feet with screw and washer when provided **(Figure** **77)**.

8. Insert casters into feet by placing stem of caster into holes provided. Apply pressure and twisting motion until casters snap into place **(Figure** **78).**

9. Repeat steps 3-8 with remaining feet. 10. Return tank to upright position.

**REAR** **WHEEL** **DOLLY/TOOL** **HOLDER** **AND** **FRONT** **CASTER** **FEET** **ASSEMBLY** **FOR** **METAL** **TANKS**

**(Not** **standard** **with** **all** **models)**

You will find two casters **(79)**, two large rear wheels **(80)**, one axle **(81)**, rear dolly **(82)**, two caster feet **(83)** and four screws with your wet/dry vacuum. Assemble as follows:

**79** **80** **81** **82** **83**

9. Insert basket (if provided) through center of carriage handle and slide into place. **ITEM** **NUMBER** **&** **DESCRIPTION**

1. Cap nut 7. #8 x 1/2" lg. Screw 2. 8" wheel 8. 1/4 - 20 x 3/4" lg. 3. Axle Machine screw 4. Rear frame 9. 1/4" Flatwasher

5. Caster socket 10. 1/4 - 20 Hex nut 6. Front frame 11. Caster

**2** **11**

**1** **5** **7**

**Tank**

**Machine** **9** **Screw**

1. With cord disconnected from receptacle and tank cover removed, turn tank upside down so that the bottom is facing up.

2. Place axle upright on a hard surface and hammer on (1) cap nut. Place (1) wheel on axle and slide down to cap nut **(Figure** **84)**. Be sure flat side of wheel hub is facing outward.

3. Slide axle through holes provided in dolly **(Figure** **85)**.

4. Slide remaining wheel onto axle and hammer on second cap nut **(Figure** **86)**.

5. With a pair of scissors, trim the enclosed template to fit your size tank. Sizes will be 11”, 14” or 16” diameters.

6. Once template is cut out, place on bottom of tank, align inlet arrow on template with center of inlet on tank **(Figure** **87)**.

7. Align cutouts in center of rear dolly with bars on template **(Figure** **88)**.

8. Place groove of rear dolly over rim of tank and push until the dolly is tight against bottom of tank **(Figure** **89)**.

9. Secure dolly with screw and washer provided **(Figure** **90)**.

10. If caster feet are attached together, separate by removing webbing.

11. Take caster foot marked with the letter A and align arrow on foot **(Figure** **91)** with arrow on template also marked with the letter A **(Figure** **92)**.

12. Place groove of foot over rim of tank and push until the caster foot is tight against bottom of tank **(Figure** **93)**.

13. Secure feet with screw and washer provided **(Figure** **94)**.

14. Insert casters into feet by placing stem of caster into holes provided. Apply pressure and twisting motion until casters snap into place **(Figure** **95).**

15. Place tool basket **(not** **standard** **with** **all** **models)**, with curved surface against tank, on rear wheel dolly assembly **(Figure** **96)**.

**8** **4**

1. Metal tank handle 2. Side tank handle

3. #10 x 3/4" Screw hex head

**3**

**5**

**Dolly**

4. Bolt 1/4 - 20 x 1/2" 5. 1/4 - 20 Hex nut

**1**

**2**

**4**

**84** **85** **86** **87** **Template**

**B** **A**

**SIDE** **TANK** **HANDLE** **ASSEMBLY**

**A** **B**

**Bottom** **of** **Tank**

**(Not** **standard** **with** **all** **models)**

Attach side handles to tank with screws provided **(Figure** **97)**.

**97**

**88** **89** **90**

**FOUR** **WHEEL** **HEAVY** **DUTY** **DOLLY** **93** **94** **95** **96** **ASSEMBLY**

**(Not** **standard** **with** **all** **models)**

**Tank** **Bottom**

**DOLLY,** **CARRIAGE** **HANDLE** **AND** **BASKET** **ASSEMBLY** **FOR** **METAL** **TANKS**

**(Not** **standard** **with** **all** **models)**

1. Remove head from tank and place tank upside down on a flat surface.

2. Place wheels on rear frame/axle assembly with extended hub of wheel towards dolly frame and place cap nuts on axle. Secure with hammer.

3. Insert caster socket into front frame and secure with phillips head screw.

4. Place groove in front frame into lip of tank and position so frame is directly above inlet. 5. Position grooves of rear frame into lip of tank and align so rear and front frames engage. 6. Secure dolly frame to tank by placing machine screws up through holes in dolly frame.

Ensure head of screw is fully recessed in area provided. After machine screw is inserted, tighten with flatwasher and hex nut.

7. Insert caster in caster socket and apply downward pressure until caster snaps into place. 8. Return vacuum to upright position. Attach carriage handle to tank by inserting bolt through

the center hole of handle and tank, secure with nut provided. Attach side handles with screws provided. Be sure to spread ends of carriage handle when assembling to prevent damage to tank.

**Tools** **required:**

(2) 1/2 inch open end wrenches, (2) 7/16 inch open end wrenches, or a socket set and a ham-mer.

1. Insert 21/2 inch long bolt through center hole in rear frame, attach split lockwasher and nut and tighten securely.

2. Attach handle brace to back of rear frame with 5/8 inch long machine screws, lockwash-ers, and nuts. (Finger tighten only.)

3. Position main frame inside rear frame. Attach (2) 5/8 inch long machine screws, lockwash-ers and nuts in both sides.Tighten securely.

4. Attach handle uprights, inside main frame (make sure buttons at top face inward) using 5/8 inch long machine screws, lockwashers and nuts. (Finger tighten only.) Align holes at top

of handle braces with holes in handle uprights. Attach with 11/4 inch long machine screws, lockwashers and nuts. (Tighten securely.)

5. Go back and tighten machine screws at bottom of uprights and braces.

6. Attach caster sockets (open end down) to front of main frame using 5/8 inch long machine screws, lockwashers and nuts. Insert casters into sockets.

7. Slide basket adapters on handle.

8. See **Figure** **98** **and** **Figure** **99** for correct installation of adapters.

9. Attach handle onto uprights by pushing down and holding buttons in on uprights. 10. Place tank retaining bracket through slot and bolt in rear frame and screw on knob. 11. Slide bumper down over main dolly frame until it bottoms out.

12. Place axle upright on a hard surface and hammer on (1) cap nut. Place (1) wheel on axle

and slide down to cap nut. Slide axle through rear of frame and slide on other wheel. Before assembling cap nut on other end of axle, be certain dolly is assembled correctly. (You may place tank on dolly and tighten knob of retaining bracket to be sure of correct assembly.)

13. After ensuring dolly is assembled correctly remove tank and place dolly on side with installed cap nut on hard surface and hammer second cap nut on axle.

14. Place accessory basket on adapters and pull out on outer rim of basket and snap into place **(Figure** **100)**.

**For** **14"** **Diameter** **Tanks**

**BAND** **DOLLY** **ASSEMBLY**

**(Not** **standard** **with** **all** **models)**

1. Place casters into sockets on band assembly.

2. Place tank upside down and slip band assembly over lip on bottom of tank. 3. Insert bolt and tighten nut until secure.

**ITEM** **NUMBER** **&** **DESCRIPTION**

**98**

**Handle** **Handle**

1. 55 Gal. band assembly 2. Caster

3. Hex head bolt, 1/4 - 20 x 13/4 4. Hex nut, 1/4 - 20

**99**

**Handle**

**Basket** **Adapter**

**For** **16"** **Diameter** **Tanks**

**Tank**

**Basket**

**Handle**

**Basket** **Adapter**

4 2

3

**FILTRATION**

**Pull** **Outward** **on** **Basket**

**100**

**ITEM** **NUMBER** **&** **DESCRIPTION**

**Keep** **Filters** **Clean**

The efficiency of these vacuum cleaners is largely dependent on the filter.

**A** **clogged** **filter** **can** **cause** **overheating** **and** **possibly** **damage** **the** **vacuum** **cleaner.**

Clean or replace filters regularly. Do not use the vacuum or filters for collecting hazardous or other health endangering materials.

**NOTE:** Never machine wash or dry filters.

**DRY** **PICK** **UP** **OPERATION**

1. Handle 12. 2. Handle upright 13. 3. Handle brace 14. 4. 1/4 - 20 x 11/4" Hex head 15.

machine screw (Black)

5. 1/4" External tooth 16. lockwasher 17.

6. 1/4 - 20 Hex nut (Black) 18. 7. Rear dolly frame 19. 8. Main dolly frame 20. 9. 5/16 - 18 x 21/2" Hex head bolt 21. 10. 5/16" Split lockwash 22. 11. 5/16 - 18 Hex nut 23.

**1**

**4**

**5**

**6**

**23**

**3**

**15** **2**

**15**

**14**

**10** **11**

**5**

**16**

**5**

Tank retainer bracket Threaded knob

Axle

1/4 - 20 x 5/8" Hex head machine screw

1/4 - 20 Hex nut Caster socket Caster

Bumper

10" Wheel (25.4cm) Cap nut

Accessory basket Basket adapter

**22**

**23**

**13**

**12**

**20**

**INSTALLING** **FOAM** **SLEEVE** **AND** **REUSABLE** **DRY** **FILTER**

**(Not** **standard** **with** **all** **models)**

**WARNING** **–** **ALWAYS** **DISCONNECT** **THE** **PLUG** **FROM** **THE** **WALL** **OUTLET** **BEFORE** **REMOVING** **THE** **TANK** **COVER.**

To pick up dust and dry material, you must install foam sleeve and reusable dry filter to ensure proper filtration. If the vacuum has been used to pick up liquids, the foam sleeve must be cleaned and dried before installing for dry pick up.

With tank cover in an upside down position, slide foam sleeve down over lid cage pulling until foam sleeve completely covers lid cage **(Figure** **101).** **NOTE:** Bottom of foam sleeve must be positioned on the OUTSIDE of groove around lid cage for the reusable dry filter to fit properly **(Figure** **102,** **103).** Center the reusable dry filter on lid cage **(Figure** **104),** slide mounting ring down over filter until ring is positioned against the ribs of the lid cage **(Figure** **105).** The reusable dry filter should always be in position over the foam sleeve for dry pick up.To remove

the filter for cleaning, remove mounting ring and filter from lid cage **(Figure** **106).** To clean the reusable dry filter, shake off excess dirt and dust or (depending on the condition of the filter) rinse with water. Allow the filter to dry completely and re-install.**DO** **NOT** **MACHINE** **WASH** **OR** **DRY.**

**IMPORTANT:** **BEFORE** **INSTALLING** **REUSABLE** **FILTER** **BE** **SURE** **THAT** **FOAM** **SLEEVE** **IS** **OUTSIDE** **OF** **GROOVE** **AND** **AROUND** **LID** **CAGE** **(Figure** **102,** **103).**

**NOTE:** **ENSURE** **THAT** **THE** **MOUNTING** **RING** **IS** **COMPLETELY** **SECURE** **AND** **IN** **POSI-TION** **BY** **PRESSING** **DOWN** **FIRMLY** **AROUND** **THE** **RING** **IN** **SEVERAL** **PLACES.** **BE** **SURE** **THE** **REUSABLE** **DRY** **DISC** **FILTER** **COMPLETELY** **COVERS** **THE** **FOAM** **SLEEVE.** **CHECK** **TO** **ENSURE** **THAT** **ALL** **EDGES** **OF** **THE** **REUSABLE** **DRY** **FILTER** **ARE** **SECURE** **UNDER** **THE** **MOUNTING** **RING.**

**CAUTION** **–** **Keep** **Filters** **Clean**

**101** **102** **103**

**19** **9** **21**

**17** **15** **8**

**15**

**18**

**104** **105** **106** **WARNING** **FOR** **FINE** **DUST** **&** **POWDERS**

**INSTALLING** **CARTRIDGE** **FILTER** **(Not** **standard** **with** **all** **models)**

**NOTE:** If foam sleeve is in position over lid cage for some models, it does not need to be removed before installing cartridge. Foam must be positioned on the INSIDE of groove around lid cage for cartridge to ﬁt properly.

The cartridge ﬁlter can be used for wet or dry pick up; installation is the same for both. When picking up large quantities of water we recommend using the foam sleeve **(not** **standard** **with** **all** **models)** in position over the lid cage. Use the cartridge ﬁlter in position over the lid cage for most general dry material pxick up. With the tank cover in an upside down position, slide the cartridge ﬁlter down over the lid cage, pushing until the ﬁlter seals against the cover **(Figure** **107).**Place ﬁlter retainer into the top of the cartridge ﬁlter, hold the tank cover with one hand, turn the handle on the ﬁlter retainer clockwise to tighten, locking the ﬁlter into place **(Figures** **108** **&** **109).**To remove the ﬁlter for cleaning, again hold the tank cover and turn the ﬁlter retainer counter-clockwise to loosen and remove, slide the cartridge ﬁlter off the lid cage **(Fig-ures** **110** **&** **111).**To clean the cartridge ﬁlter shake or brush off excess dirt or rinse (from the inside of the ﬁlter) with water, dry completely (approximately 24 hours) and re-install.**(Figures** **112).** **NOTE:** **IF** **THE** **FILTER** **HAS** **BEEN** **USED** **FOR** **WET** **PICK** **UP,** **IT** **MUST** **BE** **CLEANED** **AND** **DRIED** **BEFORE** **USING** **FOR** **DRY** **PICK** **UP.**

**INSTALLING** **THE** **DISPOSABLE** **FILTER** **BAG**

**(Not** **Standard** **with** **All** **Models)**

1. Use for dry pick up only. Use in conjunction with cartridge filter for picking up soot, cement, plaster or drywall dust.

2. With cord disconnected from receptacle, pull latches in an outward motion and remove tank cover.

3. Unscrew hose locking-nut and remove hose from inlet **(Figure** **113).**

4. Remove inlet deflector from deflector guide **(Figure** **114).** **NOTE:** Hose must be removed before inlet deflector can be taken out.

5. With the opening of the inlet deflector facing the bottom of the filter bag, slide collection bag collar over deflector matching notches of bag collar to tabs on inlet deflector, bag will only fit properly one way **(Figure** **115).**

6. Slide deflector with collection bag attached into deflector guide **(Figure** **116).** 7. Reinsert hose into inlet and tighten locking-nut **(Figure** **117).**

8. When secured in place, expand bag and position around the inside of the tank.

**Locking Inlet:**

**Friction Inlet:**

**(Not** **standard** **with** **all** **models)** 1. Use for dry pick up only.

2. With cord disconnected from receptacle, pull latches in an outward motion and remove tank cover.

3. Grasp cardboard collar ﬁrmly and slide rubber guard onto inlet ﬁtting as far as possible **(Figure** **118).**

4. When secured in place, expand bag and position around the inside of the tank **(Figure** **119).**

When vacuuming fine dust, or powders of any kind (ex. plaster, drywall dust, cold ashes, con-crete dust, etc.)...a **high** **efficiency** **drywall** **filter** **bag** **must** **be** **used**.When vacuuming normal household dust and debris, standard household disposable filter bags may be used. These "large bag" filters connect to the air inlet fitting on the inside of the vacuum tank.

**WET** **PICK** **UP** **OPERATION**

Remove ALL dirt and debris found in the tank. The vacuum requires only a minimum of con-version when going from dry to wet pick up. Remove all dry use filters from the vacuum. Wet pick up requires the foam sleeve **(not** **standard** **with** **all** **models)** or cartridge filter **(not** **stan-dard** **with** **all** **models)** to be in position over the lid cage. For proper installation instructions for wet pick up using the cartridge filter or foam sleeve, refer to Installing the Cartridge Filter. Do not use the reusable dry filter for wet pick up. Remove inlet deflector from the deflector guide sliding in an upward motion. **NOTE:** Hose must be removed before inlet deflector can be taken out. Reinstall being sure the opening of the inlet deflector is facing the top of the tank misting may occur if inlet deflector is not inserted properly. Misting in exhaust air may occur if the filter becomes saturated during wet pick up If misting occurs, remove filter and allow to dry or, replace with another dry filter to eliminate the misting and possible dripping of liquid around the lid. Turn the unit off immediately upon completing a wet pick up job or when tank is full and ready to be emptied. Raise the hose to drain any excess liquid into the tank.The interior of the tank should be periodically cleaned.

The foam sleeve should be cleaned periodically as described in the following steps:

1.Always disconnect the plug from the wall receptacle before removing the tank cover. Place tank cover in an upside down position. Remove foam sleeve by sliding it up and off the lid cage.

2.Shake excess dust off foam sleeve with a rapid up and down movement.

3.Hold foam sleeve under running water for a minute or two, rinsing from the inside. A water wash is not always required, depending on the condition of the foam sleeve.

4.Gently wring out excess water, blot foam sleeve with a clean towel, and allow to dry.The foam sleeve is now ready to be reinstalled on the lid cage.

**NOTE:** **WET** **PICK** **UP** **ACCESSORIES** **SHOULD** **BE** **WASHED** **PERIODICALLY,** **ESPECIALLY** **AFTER** **PICKING** **UP** **WET,** **STICKY** **KITCHEN** **ACCIDENTS.** **THIS** **CAN** **BE** **ACCOMPLISHED** **WITH** **A** **WARM** **SOLUTION** **OF** **SOAP** **AND** **WATER.**

**OPERATION**

**This** **equipment** **incorporates** **parts** **such** **as** **switches,** **motors** **or** **the** **like** **that** **tend** **to** **produce** **arcs** **or** **sparks** **that** **can** **cause** **an** **explosion.** **Do** **not** **pick** **up** **flammable,** **combustible,** **or** **hot** **materials.** **Do** **not** **use** **around** **explosive** **liquids** **or** **vapors,** **as** **electrical** **devices** **produce** **arcs** **or** **sparks** **which** **can** **cause** **a** **fire** **or** **explosion** **-** **do** **not** **use** **at** **filling** **stations** **or** **anywhere** **gasoline** **is** **stored** **or** **dispensed.**

**WARNING**² **IF** **ANY** **OF** **THE** **MOTOR** **HOUSING** **PARTS** **SHOULD** **BECOME** **DETACHED** **OR** **BROKEN,** **EXPOSING** **THE** **MOTOR**

**OR** **ANY** **OTHER** **ELECTRICAL** **COMPONENTS,** **OPERATION** **SHOULD** **BE** **DISCONTINUED** **IMMEDIATELY** **TO** **AVOID** **PERSONAL** **INJURY** **OR** **FURTHER** **DAMAGE** **TO** **THE** **VACUUM.** **REPAIRS** **SHOULD** **BE** **MADE** **BEFORE** **REUSING** **THE** **VACUUM.**

**BLOWER** **FEATURE** **Blower** **Use**

Some vacuum cleaners can be used as a powerful blower by inserting the hose into the motor housing exhaust port.

**118** **119**

**ALWAYS** **WEAR** **EYE** **PROTECTION** **TO** **PREVENT** **ROCKS** **OR** **DEBRIS** **FROM** **BEING** **BLOWN** **OR** **RICOCHETING** **INTO** **THE** **EYES** **OR** **FACE** **WHICH** **CAN** **RESULT** **IN** **SERIOUS** **INJURY.**

Your vacuum can be used as a powerful blower. To use your unit as a blower, clear hose of any obstruc-tion. Insert machine hose end into blower port on rear of unit **(Figure** **120,** **121)**. Twist slightly to tighten the connection. Caution should be used when using as a blower due to the powerful force of air when using certain attachments.

**EMPTYING** **LIQUID** **WASTES** **FROM** **THE** **TANK** ***1RWDOOXQLWVDUHHTXLSSHGZLWKWDQNGUDLQV)ROORZWKHLQVWUXFWLRQV*** ***ZKLFKDSSO\WR\RXUVSHFLILFXQLW***

**Without** **Tank** **Drain**

Liquid waste may be emptied by removing the tank cover. To empty, stop the motor and remove the plug from the wall receptacle. Remove the tank cover and deposit the liquid waste contents in a suitable drain. After tank is empty, return the cover to its original position. To continue use, plug the cord into the wall receptacle and turn the unit on.

**With** **Tank** **Drain**

Liquid waste may be emptied by removing the tank drain. To empty, turn unit off and remove plug from wall receptacle. Remove the drain cap and deposit the liquid waste contents in a suitable drain. After the tank is empty, return the drain cap to its original position. To continue use, plug the cord into the wall receptacle and turn the unit on.

**AUTOMATIC** **SUCTION** **SHUT-OFF**

The vacuum is equipped with an automatic suction shut-off that operates when picking up liq-uids. As the level of the liquid rises in the tank, an internal float rises until it seats itself against a seal at the intake of the motor, shutting off suction. When this happens, the motor will develop a higher than normal pitch noise and the suction is drastically reduced. If this occurs, turn unit off immediately. Failure to turn unit off after float rises and shuts off suction will result in extensive damage to the motor. To continue use, empty the liquid waste from the tank as outlined in the previous paragraph.

**NOTE:** IF ACCIDENTALLY TIPPED OVER, THE VACUUM COULD LOSE SUCTION. IF

THIS OCCURS, PLACE VAC IN UPRIGHT POSITION AND TURN SWITCH OFF.THIS WILL ALLOW THE FLOAT TO RETURN TO ITS NORMAL POSITION, AND YOU WILL BE ABLE TO CONTINUE OPERATION.

**LUBRICATION**

No lubrication is necessary as the motor is equipped with lifetime lubricated bearings.

**STORAGE**

Before storing your vacuum cleaner the tank should be emptied and cleaned. **122** The power cord can be wrapped around the cord wraps provided on the

tank cover on rear or side of unit **(Figure** **122,** **123,** **124).** Accessories may be stored in the tool holder **(not** **standard** **on** **all** **models)** so they can be readily available.**The** **vacuum** **should** **be** **stored** **indoors.**

**123** **124**

**ACCESSORIES,** **HOSES** **AND** **WANDS**

All Shop-Vac® vacuums covered in this manual come with accessories to cover wet and dry cleanup jobs. Not all vacs include all accessories shown.

**Nozzles** **and** **Accessories** **Hoses** **Wands**

**Lock**

**Lock**

**Carpet** **Tool** **Insert**

**Double** **Blade** **Squeegee** **Insert**

**Floor** **Brush** **Insert**

**All** **Friction** **Fit** **Accessories**

**Insert** **wand** **end** **or** **hose** **into** **accessory** **and** **twist** **to**

**form** **a** **tight** **fit.**

**Insert** **machine** **hose** **end** **into** **tank** **and** **twist** **to** **form** **a**

**tight** **fit.**

**All** **Friction** **Fit** **Wands** **Insert** **wand** **ends** **together**

**and** **twist** **to** **form** **a** **tight** **fit.**

**Inserts** **lock** **into** **place** **by**

**sliding** **red** **buttons.** **Elbow** **swivels**

**Carpet** **Tool**

**Insert** **Squeegee** **Insert**

**Brush** **Insert** **Shown** **Inserts** **lock** **into** **place** **by**

**sliding** **insert** **onto** **nozzle.**

**Posi-Lock** **Hoses** **Insert** **hose** **collar** **onto** **threaded** **tank** **inlet** **and**

**tighten.**

**Positive** **Locking** **Wands** **Insert** **wand** **ends** **together**

**until** **metal** **push** **button** **locks.**

**Inserts** **snap-in** **and** **out.**

**Elbow** **swivels.**

**Levers** **control** **brush** **position** **for**

**various** **types** **of** **cleaning.**

**Locking** **Nut** **Wand** **End** **Insert** **wand** **end** **over** **nozzle**

**and** **tighten** **nut.**

**SHOP-VAC®** **VACUUM** **FILTER** **CLEANING** **REFERENCE**

**Foam** **Sleeve**

Rinse with water, dry and reinstall.

**Reusable** **Disc** **Filter**

Rinse with water, dry and reinstall; do not machine wash.

**Super** **Performance** **Filter** **Full** **Polyester** **Filter** Dispose of after filter develops rips or tears. Brush off dirt and reinstall; if filter gets wet,

rinse with water, dry and reinstall.

**All** **Collection** **Bags** **Ultra** **Web®** **Cartridge** **Filters** Dispose of bag when full. From inside of filter, rinse with water, dry com-

pletely and reinstall.

**Cleanstream®** **Cartridge** **Filters**

Clean installed filter by simply tapping or shaking the vacuum unit.To restore optimum airflow, remove filter, tap end cap against

a hard surface to loosen debris. Additional debris can be removed by rinsing outside surface of filter with running water. Avoid dampening inside of filter. Completely air dry filter after washing.

**Troubleshooting** **Chart** **Symptom** **Parts/accessories** **missing**

**Vacuum** **cleaner** **will** **not** **start**

**Dust** **discharging** **from** **exhaust**

**Loss** **of** **suction**

**Static** **shock**

**Possible** **Cause(s)** 1. Packed in tank

1. No power at receptacle 2. Defective switch

3. Defective motor

1. Filter not installed/not installed properly 2. Filter damaged

3. Filter clogged or dust is too fine 4. Filter not functional

1. Loose hose connection 2. Filter clogged

3. Full tank

4. Hole in hose

1. Dry environment

2. Relative humidity of air is low

**Corrective** **Action** 1. Check in tank

1. Check for power 2. Replace switch 3. Replace motor

1. Properly install filter 2. Replace filter

3. Use more efficient filter 4. Clean and replace filter

1.Tighten hose connection 2. Clean or replace filter

3. Empty tank 4. Replace hose

1.Add moisture to air (if practical, use a console or installed humidifier).

2.This situation is temporary and does not affect the use of the vacuum cleaner.

McGrp.Ru

Сайт техники и электроники

Наш сайт [McGrp.Ru](http://mcgrp.ru/) при этом не является просто хранилищем

[инструкций по эксплуатации,](http://mcgrp.ru/) это живое сообщество людей. Они общаются

на форуме, задают вопросы о способах и особенностях использования техники. На все вопросы очень быстро находятся ответы от таких же посетителей сайта, экспертов или администраторов. Вопрос можно задать как на форуме, так и

в специальной форме на странице, где описывается интересующая вас техника.